F439_CPP_TX-RX_LoRa_Project

Loading...
Searching...
No Matches
Data Fields
SX1262_IrqResult Struct Reference

IRQ processing result and optional received payload data. More...

`#include <sx1262.h>`

## Data Fields
bool | rx_done
bool | tx_done
bool | crc_error
bool | timeout
int8_t | rssi_pkt
int8_t | snr_pkt
uint8_t | payload [256]
uint8_t | payload_len

## Detailed Description

IRQ processing result and optional received payload data.

## Field Documentation

## ◆ crc_error

bool SX1262_IrqResult::crc_error

## ◆ payload

uint8_t SX1262_IrqResult::payload[256]

## ◆ payload_len

uint8_t SX1262_IrqResult::payload_len

## ◆ rssi_pkt

int8_t SX1262_IrqResult::rssi_pkt

## ◆ rx_done

bool SX1262_IrqResult::rx_done

## ◆ snr_pkt

int8_t SX1262_IrqResult::snr_pkt

## ◆ timeout

bool SX1262_IrqResult::timeout

## ◆ tx_done

bool SX1262_IrqResult::tx_done

The documentation for this struct was generated from the following file:

- SX1262/sx1262.h