F439_CPP_TX-RX_LoRa_Project

Loading...
Searching...
No Matches
stm32f4xx_hal_conf.h
Go to the documentation of this file.
1/* USER CODE BEGIN Header */
21/* USER CODE END Header */
22
23/* Define to prevent recursive inclusion -------------------------------------*/
24#ifndef __STM32F4xx_HAL_CONF_H
25#define __STM32F4xx_HAL_CONF_H
26
27#ifdef __cplusplus
28 extern "C" {
29#endif
30
31/* Exported types ------------------------------------------------------------*/
32/* Exported constants --------------------------------------------------------*/
33
34/* ########################## Module Selection ############################## */
38#define HAL_MODULE_ENABLED
39
40 #define HAL_CRYP_MODULE_ENABLED
41/* #define HAL_ADC_MODULE_ENABLED */
42/* #define HAL_CAN_MODULE_ENABLED */
43/* #define HAL_CRC_MODULE_ENABLED */
44/* #define HAL_CAN_LEGACY_MODULE_ENABLED */
45/* #define HAL_DAC_MODULE_ENABLED */
46/* #define HAL_DCMI_MODULE_ENABLED */
47/* #define HAL_DMA2D_MODULE_ENABLED */
48/* #define HAL_ETH_MODULE_ENABLED */
49/* #define HAL_ETH_LEGACY_MODULE_ENABLED */
50/* #define HAL_NAND_MODULE_ENABLED */
51/* #define HAL_NOR_MODULE_ENABLED */
52/* #define HAL_PCCARD_MODULE_ENABLED */
53/* #define HAL_SRAM_MODULE_ENABLED */
54/* #define HAL_SDRAM_MODULE_ENABLED */
55/* #define HAL_HASH_MODULE_ENABLED */
56/* #define HAL_I2C_MODULE_ENABLED */
57/* #define HAL_I2S_MODULE_ENABLED */
58/* #define HAL_IWDG_MODULE_ENABLED */
59/* #define HAL_LTDC_MODULE_ENABLED */
60/* #define HAL_RNG_MODULE_ENABLED */
61/* #define HAL_RTC_MODULE_ENABLED */
62/* #define HAL_SAI_MODULE_ENABLED */
63/* #define HAL_SD_MODULE_ENABLED */
64/* #define HAL_MMC_MODULE_ENABLED */
65#define HAL_SPI_MODULE_ENABLED
66#define HAL_TIM_MODULE_ENABLED
67#define HAL_UART_MODULE_ENABLED
68/* #define HAL_USART_MODULE_ENABLED */
69/* #define HAL_IRDA_MODULE_ENABLED */
70/* #define HAL_SMARTCARD_MODULE_ENABLED */
71/* #define HAL_SMBUS_MODULE_ENABLED */
72/* #define HAL_WWDG_MODULE_ENABLED */
73/* #define HAL_PCD_MODULE_ENABLED */
74/* #define HAL_HCD_MODULE_ENABLED */
75/* #define HAL_DSI_MODULE_ENABLED */
76/* #define HAL_QSPI_MODULE_ENABLED */
77/* #define HAL_QSPI_MODULE_ENABLED */
78/* #define HAL_CEC_MODULE_ENABLED */
79/* #define HAL_FMPI2C_MODULE_ENABLED */
80/* #define HAL_FMPSMBUS_MODULE_ENABLED */
81/* #define HAL_SPDIFRX_MODULE_ENABLED */
82/* #define HAL_DFSDM_MODULE_ENABLED */
83/* #define HAL_LPTIM_MODULE_ENABLED */
84#define HAL_GPIO_MODULE_ENABLED
85#define HAL_EXTI_MODULE_ENABLED
86#define HAL_DMA_MODULE_ENABLED
87#define HAL_RCC_MODULE_ENABLED
88#define HAL_FLASH_MODULE_ENABLED
89#define HAL_PWR_MODULE_ENABLED
90#define HAL_CORTEX_MODULE_ENABLED
91
92/* ########################## HSE/HSI Values adaptation ##################### */
98#if !defined (HSE_VALUE)
99 #define HSE_VALUE 8000000U
100#endif /* HSE_VALUE */
101
102#if !defined (HSE_STARTUP_TIMEOUT)
103 #define HSE_STARTUP_TIMEOUT 100U
104#endif /* HSE_STARTUP_TIMEOUT */
105
111#if !defined (HSI_VALUE)
112 #define HSI_VALUE ((uint32_t)16000000U)
113#endif /* HSI_VALUE */
114
118#if !defined (LSI_VALUE)
119 #define LSI_VALUE 32000U
120#endif /* LSI_VALUE */
126#if !defined (LSE_VALUE)
127 #define LSE_VALUE 32768U
128#endif /* LSE_VALUE */
129
130#if !defined (LSE_STARTUP_TIMEOUT)
131 #define LSE_STARTUP_TIMEOUT 5000U
132#endif /* LSE_STARTUP_TIMEOUT */
133
139#if !defined (EXTERNAL_CLOCK_VALUE)
140 #define EXTERNAL_CLOCK_VALUE 12288000U
141#endif /* EXTERNAL_CLOCK_VALUE */
142
143/* Tip: To avoid modifying this file each time you need to use different HSE,
144 === you can define the HSE value in your toolchain compiler preprocessor. */
145
146/* ########################### System Configuration ######################### */
150#define VDD_VALUE 3300U
151#define TICK_INT_PRIORITY 0U
152#define USE_RTOS 0U
153#define PREFETCH_ENABLE 1U
154#define INSTRUCTION_CACHE_ENABLE 1U
155#define DATA_CACHE_ENABLE 1U
156
157#define USE_HAL_ADC_REGISTER_CALLBACKS 0U /* ADC register callback disabled */
158#define USE_HAL_CAN_REGISTER_CALLBACKS 0U /* CAN register callback disabled */
159#define USE_HAL_CEC_REGISTER_CALLBACKS 0U /* CEC register callback disabled */
160#define USE_HAL_CRYP_REGISTER_CALLBACKS 0U /* CRYP register callback disabled */
161#define USE_HAL_DAC_REGISTER_CALLBACKS 0U /* DAC register callback disabled */
162#define USE_HAL_DCMI_REGISTER_CALLBACKS 0U /* DCMI register callback disabled */
163#define USE_HAL_DFSDM_REGISTER_CALLBACKS 0U /* DFSDM register callback disabled */
164#define USE_HAL_DMA2D_REGISTER_CALLBACKS 0U /* DMA2D register callback disabled */
165#define USE_HAL_DSI_REGISTER_CALLBACKS 0U /* DSI register callback disabled */
166#define USE_HAL_ETH_REGISTER_CALLBACKS 0U /* ETH register callback disabled */
167#define USE_HAL_HASH_REGISTER_CALLBACKS 0U /* HASH register callback disabled */
168#define USE_HAL_HCD_REGISTER_CALLBACKS 0U /* HCD register callback disabled */
169#define USE_HAL_I2C_REGISTER_CALLBACKS 0U /* I2C register callback disabled */
170#define USE_HAL_FMPI2C_REGISTER_CALLBACKS 0U /* FMPI2C register callback disabled */
171#define USE_HAL_FMPSMBUS_REGISTER_CALLBACKS 0U /* FMPSMBUS register callback disabled */
172#define USE_HAL_I2S_REGISTER_CALLBACKS 0U /* I2S register callback disabled */
173#define USE_HAL_IRDA_REGISTER_CALLBACKS 0U /* IRDA register callback disabled */
174#define USE_HAL_LPTIM_REGISTER_CALLBACKS 0U /* LPTIM register callback disabled */
175#define USE_HAL_LTDC_REGISTER_CALLBACKS 0U /* LTDC register callback disabled */
176#define USE_HAL_MMC_REGISTER_CALLBACKS 0U /* MMC register callback disabled */
177#define USE_HAL_NAND_REGISTER_CALLBACKS 0U /* NAND register callback disabled */
178#define USE_HAL_NOR_REGISTER_CALLBACKS 0U /* NOR register callback disabled */
179#define USE_HAL_PCCARD_REGISTER_CALLBACKS 0U /* PCCARD register callback disabled */
180#define USE_HAL_PCD_REGISTER_CALLBACKS 0U /* PCD register callback disabled */
181#define USE_HAL_QSPI_REGISTER_CALLBACKS 0U /* QSPI register callback disabled */
182#define USE_HAL_RNG_REGISTER_CALLBACKS 0U /* RNG register callback disabled */
183#define USE_HAL_RTC_REGISTER_CALLBACKS 0U /* RTC register callback disabled */
184#define USE_HAL_SAI_REGISTER_CALLBACKS 0U /* SAI register callback disabled */
185#define USE_HAL_SD_REGISTER_CALLBACKS 0U /* SD register callback disabled */
186#define USE_HAL_SMARTCARD_REGISTER_CALLBACKS 0U /* SMARTCARD register callback disabled */
187#define USE_HAL_SDRAM_REGISTER_CALLBACKS 0U /* SDRAM register callback disabled */
188#define USE_HAL_SRAM_REGISTER_CALLBACKS 0U /* SRAM register callback disabled */
189#define USE_HAL_SPDIFRX_REGISTER_CALLBACKS 0U /* SPDIFRX register callback disabled */
190#define USE_HAL_SMBUS_REGISTER_CALLBACKS 0U /* SMBUS register callback disabled */
191#define USE_HAL_SPI_REGISTER_CALLBACKS 0U /* SPI register callback disabled */
192#define USE_HAL_TIM_REGISTER_CALLBACKS 0U /* TIM register callback disabled */
193#define USE_HAL_UART_REGISTER_CALLBACKS 0U /* UART register callback disabled */
194#define USE_HAL_USART_REGISTER_CALLBACKS 0U /* USART register callback disabled */
195#define USE_HAL_WWDG_REGISTER_CALLBACKS 0U /* WWDG register callback disabled */
196
197/* ########################## Assert Selection ############################## */
202 #define USE_FULL_ASSERT 1U
203
204/* ################## Ethernet peripheral configuration ##################### */
205
206/* Section 1 : Ethernet peripheral configuration */
207
208/* MAC ADDRESS: MAC_ADDR0:MAC_ADDR1:MAC_ADDR2:MAC_ADDR3:MAC_ADDR4:MAC_ADDR5 */
209#define MAC_ADDR0 2U
210#define MAC_ADDR1 0U
211#define MAC_ADDR2 0U
212#define MAC_ADDR3 0U
213#define MAC_ADDR4 0U
214#define MAC_ADDR5 0U
215
216/* Definition of the Ethernet driver buffers size and count */
217#define ETH_RX_BUF_SIZE ETH_MAX_PACKET_SIZE /* buffer size for receive */
218#define ETH_TX_BUF_SIZE ETH_MAX_PACKET_SIZE /* buffer size for transmit */
219#define ETH_RXBUFNB 4U /* 4 Rx buffers of size ETH_RX_BUF_SIZE */
220#define ETH_TXBUFNB 4U /* 4 Tx buffers of size ETH_TX_BUF_SIZE */
221
222/* Section 2: PHY configuration section */
223
224/* DP83848_PHY_ADDRESS Address*/
225#define DP83848_PHY_ADDRESS
226/* PHY Reset delay these values are based on a 1 ms Systick interrupt*/
227#define PHY_RESET_DELAY 0x000000FFU
228/* PHY Configuration delay */
229#define PHY_CONFIG_DELAY 0x00000FFFU
230
231#define PHY_READ_TO 0x0000FFFFU
232#define PHY_WRITE_TO 0x0000FFFFU
233
234/* Section 3: Common PHY Registers */
235
236#define PHY_BCR ((uint16_t)0x0000U)
237#define PHY_BSR ((uint16_t)0x0001U)
239#define PHY_RESET ((uint16_t)0x8000U)
240#define PHY_LOOPBACK ((uint16_t)0x4000U)
241#define PHY_FULLDUPLEX_100M ((uint16_t)0x2100U)
242#define PHY_HALFDUPLEX_100M ((uint16_t)0x2000U)
243#define PHY_FULLDUPLEX_10M ((uint16_t)0x0100U)
244#define PHY_HALFDUPLEX_10M ((uint16_t)0x0000U)
245#define PHY_AUTONEGOTIATION ((uint16_t)0x1000U)
246#define PHY_RESTART_AUTONEGOTIATION ((uint16_t)0x0200U)
247#define PHY_POWERDOWN ((uint16_t)0x0800U)
248#define PHY_ISOLATE ((uint16_t)0x0400U)
250#define PHY_AUTONEGO_COMPLETE ((uint16_t)0x0020U)
251#define PHY_LINKED_STATUS ((uint16_t)0x0004U)
252#define PHY_JABBER_DETECTION ((uint16_t)0x0002U)
254/* Section 4: Extended PHY Registers */
255#define PHY_SR ((uint16_t))
257#define PHY_SPEED_STATUS ((uint16_t))
258#define PHY_DUPLEX_STATUS ((uint16_t))
260/* ################## SPI peripheral configuration ########################## */
261
262/* CRC FEATURE: Use to activate CRC feature inside HAL SPI Driver
263* Activated: CRC code is present inside driver
264* Deactivated: CRC code cleaned from driver
265*/
266
267#define USE_SPI_CRC 0U
268
269/* Includes ------------------------------------------------------------------*/
274#ifdef HAL_RCC_MODULE_ENABLED
275 #include "stm32f4xx_hal_rcc.h"
276#endif /* HAL_RCC_MODULE_ENABLED */
277
278#ifdef HAL_GPIO_MODULE_ENABLED
279 #include "stm32f4xx_hal_gpio.h"
280#endif /* HAL_GPIO_MODULE_ENABLED */
281
282#ifdef HAL_EXTI_MODULE_ENABLED
283 #include "stm32f4xx_hal_exti.h"
284#endif /* HAL_EXTI_MODULE_ENABLED */
285
286#ifdef HAL_DMA_MODULE_ENABLED
287 #include "stm32f4xx_hal_dma.h"
288#endif /* HAL_DMA_MODULE_ENABLED */
289
290#ifdef HAL_CORTEX_MODULE_ENABLED
291 #include "stm32f4xx_hal_cortex.h"
292#endif /* HAL_CORTEX_MODULE_ENABLED */
293
294#ifdef HAL_ADC_MODULE_ENABLED
295 #include "stm32f4xx_hal_adc.h"
296#endif /* HAL_ADC_MODULE_ENABLED */
297
298#ifdef HAL_CAN_MODULE_ENABLED
299 #include "stm32f4xx_hal_can.h"
300#endif /* HAL_CAN_MODULE_ENABLED */
301
302#ifdef HAL_CAN_LEGACY_MODULE_ENABLED
303 #include "stm32f4xx_hal_can_legacy.h"
304#endif /* HAL_CAN_LEGACY_MODULE_ENABLED */
305
306#ifdef HAL_CRC_MODULE_ENABLED
307 #include "stm32f4xx_hal_crc.h"
308#endif /* HAL_CRC_MODULE_ENABLED */
309
310#ifdef HAL_CRYP_MODULE_ENABLED
311 #include "stm32f4xx_hal_cryp.h"
312#endif /* HAL_CRYP_MODULE_ENABLED */
313
314#ifdef HAL_DMA2D_MODULE_ENABLED
315 #include "stm32f4xx_hal_dma2d.h"
316#endif /* HAL_DMA2D_MODULE_ENABLED */
317
318#ifdef HAL_DAC_MODULE_ENABLED
319 #include "stm32f4xx_hal_dac.h"
320#endif /* HAL_DAC_MODULE_ENABLED */
321
322#ifdef HAL_DCMI_MODULE_ENABLED
323 #include "stm32f4xx_hal_dcmi.h"
324#endif /* HAL_DCMI_MODULE_ENABLED */
325
326#ifdef HAL_ETH_MODULE_ENABLED
327 #include "stm32f4xx_hal_eth.h"
328#endif /* HAL_ETH_MODULE_ENABLED */
329
330#ifdef HAL_ETH_LEGACY_MODULE_ENABLED
331 #include "stm32f4xx_hal_eth_legacy.h"
332#endif /* HAL_ETH_LEGACY_MODULE_ENABLED */
333
334#ifdef HAL_FLASH_MODULE_ENABLED
335 #include "stm32f4xx_hal_flash.h"
336#endif /* HAL_FLASH_MODULE_ENABLED */
337
338#ifdef HAL_SRAM_MODULE_ENABLED
339 #include "stm32f4xx_hal_sram.h"
340#endif /* HAL_SRAM_MODULE_ENABLED */
341
342#ifdef HAL_NOR_MODULE_ENABLED
343 #include "stm32f4xx_hal_nor.h"
344#endif /* HAL_NOR_MODULE_ENABLED */
345
346#ifdef HAL_NAND_MODULE_ENABLED
347 #include "stm32f4xx_hal_nand.h"
348#endif /* HAL_NAND_MODULE_ENABLED */
349
350#ifdef HAL_PCCARD_MODULE_ENABLED
351 #include "stm32f4xx_hal_pccard.h"
352#endif /* HAL_PCCARD_MODULE_ENABLED */
353
354#ifdef HAL_SDRAM_MODULE_ENABLED
355 #include "stm32f4xx_hal_sdram.h"
356#endif /* HAL_SDRAM_MODULE_ENABLED */
357
358#ifdef HAL_HASH_MODULE_ENABLED
359 #include "stm32f4xx_hal_hash.h"
360#endif /* HAL_HASH_MODULE_ENABLED */
361
362#ifdef HAL_I2C_MODULE_ENABLED
363 #include "stm32f4xx_hal_i2c.h"
364#endif /* HAL_I2C_MODULE_ENABLED */
365
366#ifdef HAL_SMBUS_MODULE_ENABLED
367 #include "stm32f4xx_hal_smbus.h"
368#endif /* HAL_SMBUS_MODULE_ENABLED */
369
370#ifdef HAL_I2S_MODULE_ENABLED
371 #include "stm32f4xx_hal_i2s.h"
372#endif /* HAL_I2S_MODULE_ENABLED */
373
374#ifdef HAL_IWDG_MODULE_ENABLED
375 #include "stm32f4xx_hal_iwdg.h"
376#endif /* HAL_IWDG_MODULE_ENABLED */
377
378#ifdef HAL_LTDC_MODULE_ENABLED
379 #include "stm32f4xx_hal_ltdc.h"
380#endif /* HAL_LTDC_MODULE_ENABLED */
381
382#ifdef HAL_PWR_MODULE_ENABLED
383 #include "stm32f4xx_hal_pwr.h"
384#endif /* HAL_PWR_MODULE_ENABLED */
385
386#ifdef HAL_RNG_MODULE_ENABLED
387 #include "stm32f4xx_hal_rng.h"
388#endif /* HAL_RNG_MODULE_ENABLED */
389
390#ifdef HAL_RTC_MODULE_ENABLED
391 #include "stm32f4xx_hal_rtc.h"
392#endif /* HAL_RTC_MODULE_ENABLED */
393
394#ifdef HAL_SAI_MODULE_ENABLED
395 #include "stm32f4xx_hal_sai.h"
396#endif /* HAL_SAI_MODULE_ENABLED */
397
398#ifdef HAL_SD_MODULE_ENABLED
399 #include "stm32f4xx_hal_sd.h"
400#endif /* HAL_SD_MODULE_ENABLED */
401
402#ifdef HAL_SPI_MODULE_ENABLED
403 #include "stm32f4xx_hal_spi.h"
404#endif /* HAL_SPI_MODULE_ENABLED */
405
406#ifdef HAL_TIM_MODULE_ENABLED
407 #include "stm32f4xx_hal_tim.h"
408#endif /* HAL_TIM_MODULE_ENABLED */
409
410#ifdef HAL_UART_MODULE_ENABLED
411 #include "stm32f4xx_hal_uart.h"
412#endif /* HAL_UART_MODULE_ENABLED */
413
414#ifdef HAL_USART_MODULE_ENABLED
415 #include "stm32f4xx_hal_usart.h"
416#endif /* HAL_USART_MODULE_ENABLED */
417
418#ifdef HAL_IRDA_MODULE_ENABLED
419 #include "stm32f4xx_hal_irda.h"
420#endif /* HAL_IRDA_MODULE_ENABLED */
421
422#ifdef HAL_SMARTCARD_MODULE_ENABLED
423 #include "stm32f4xx_hal_smartcard.h"
424#endif /* HAL_SMARTCARD_MODULE_ENABLED */
425
426#ifdef HAL_WWDG_MODULE_ENABLED
427 #include "stm32f4xx_hal_wwdg.h"
428#endif /* HAL_WWDG_MODULE_ENABLED */
429
430#ifdef HAL_PCD_MODULE_ENABLED
431 #include "stm32f4xx_hal_pcd.h"
432#endif /* HAL_PCD_MODULE_ENABLED */
433
434#ifdef HAL_HCD_MODULE_ENABLED
435 #include "stm32f4xx_hal_hcd.h"
436#endif /* HAL_HCD_MODULE_ENABLED */
437
438#ifdef HAL_DSI_MODULE_ENABLED
439 #include "stm32f4xx_hal_dsi.h"
440#endif /* HAL_DSI_MODULE_ENABLED */
441
442#ifdef HAL_QSPI_MODULE_ENABLED
443 #include "stm32f4xx_hal_qspi.h"
444#endif /* HAL_QSPI_MODULE_ENABLED */
445
446#ifdef HAL_CEC_MODULE_ENABLED
447 #include "stm32f4xx_hal_cec.h"
448#endif /* HAL_CEC_MODULE_ENABLED */
449
450#ifdef HAL_FMPI2C_MODULE_ENABLED
451 #include "stm32f4xx_hal_fmpi2c.h"
452#endif /* HAL_FMPI2C_MODULE_ENABLED */
453
454#ifdef HAL_FMPSMBUS_MODULE_ENABLED
455 #include "stm32f4xx_hal_fmpsmbus.h"
456#endif /* HAL_FMPSMBUS_MODULE_ENABLED */
457
458#ifdef HAL_SPDIFRX_MODULE_ENABLED
459 #include "stm32f4xx_hal_spdifrx.h"
460#endif /* HAL_SPDIFRX_MODULE_ENABLED */
461
462#ifdef HAL_DFSDM_MODULE_ENABLED
463 #include "stm32f4xx_hal_dfsdm.h"
464#endif /* HAL_DFSDM_MODULE_ENABLED */
465
466#ifdef HAL_LPTIM_MODULE_ENABLED
467 #include "stm32f4xx_hal_lptim.h"
468#endif /* HAL_LPTIM_MODULE_ENABLED */
469
470#ifdef HAL_MMC_MODULE_ENABLED
471 #include "stm32f4xx_hal_mmc.h"
472#endif /* HAL_MMC_MODULE_ENABLED */
473
474/* Exported macro ------------------------------------------------------------*/
475#ifdef USE_FULL_ASSERT
484 #define assert_param(expr) ((expr) ? (void)0U : assert_failed((uint8_t *)__FILE__, __LINE__))
485/* Exported functions ------------------------------------------------------- */
486 void assert_failed(uint8_t* file, uint32_t line);
487#else
488 #define assert_param(expr) ((void)0U)
489#endif /* USE_FULL_ASSERT */
490
491#ifdef __cplusplus
492}
493#endif
494
495#endif /* __STM32F4xx_HAL_CONF_H */
assert_failed
void assert_failed(uint8_t *file, uint32_t line)