<map id="Firmware Architecture" name="Firmware Architecture">
<area shape="rect" id="Node000001" title="Top&#45;level subsystem grouping for the project firmware." alt="" coords="5,119,172,145"/>
<area shape="rect" id="Node000006" href="$group__HardwareAbstractionLayer.html" title="Board&#45;level startup, HAL integration, and platform glue." alt="" coords="227,5,389,45"/>
<area shape="rect" id="Node000005" href="$group__PersistenceLayer.html" title="SPI FRAM persistence support for replay&#45;related state." alt="" coords="239,70,377,95"/>
<area shape="rect" id="Node000002" href="$group__RadioApplicationLayer.html" title="Application&#45;level radio orchestration and node behavior." alt="" coords="220,119,396,145"/>
<area shape="rect" id="Node000003" href="$group__RadioLinkProtocolLayer.html" title="Transport&#45;agnostic framing, crypto, replay protection, and wire&#45;format logic." alt="" coords="237,169,379,209"/>
<area shape="rect" id="Node000004" href="$group__SX1262DriverLayer.html" title="Hardware driver for SX1262 modem control and packet I/O." alt="" coords="231,234,385,259"/>
</map>
