F439_CPP_TX-RX_LoRa_Project

Loading...
Searching...
No Matches
Files
Persistence Layer
Firmware Architecture

SPI FRAM persistence support for replay-related state. More...

Collaboration diagram for Persistence Layer:

## Files
file | ada1897_mb85rs64b.c
| MB85RS64B SPI FRAM driver implementation.
file | ada1897_mb85rs64b.h
| MB85RS64B SPI FRAM public interface.

## Detailed Description

SPI FRAM persistence support for replay-related state.