F439_CPP_TX-RX_LoRa_Project

Loading...
Searching...
No Matches
Functions
radio_app.h File Reference
Firmware Architecture » Radio Application Layer

Application-layer radio orchestration entry points. More...

`#include "main.h"`
`#include "sx1262.h"`
Include dependency graph for radio_app.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Functions
void | RadioApp_Init (SX1262_Handle *sx)
| Initialize the radio application state.
void | RadioApp_Loop (void)
| Run one iteration of the radio application loop.
void | RadioApp_OnDio1Exti (uint16_t pin)
| Notify the application of an SX1262 DIO1 EXTI event.

## Detailed Description

Application-layer radio orchestration entry points.

## Function Documentation

## ◆ RadioApp_Init()

void RadioApp_Init | ( | SX1262_Handle * | sx | ) |

Initialize the radio application state.

Parameters

  sx | Driver handle used by the application.

Initialize the radio application state.

## ◆ RadioApp_Loop()

void RadioApp_Loop | ( | void |  | ) |

Run one iteration of the radio application loop.

Run one iteration of the radio application loop.

## ◆ RadioApp_OnDio1Exti()

void RadioApp_OnDio1Exti | ( | uint16_t | pin | ) |

Notify the application of an SX1262 DIO1 EXTI event.

Parameters

  pin | GPIO pin value reported by the EXTI callback.

Notify the application of an SX1262 DIO1 EXTI event.