F439_CPP_TX-RX_LoRa_Project

Loading...
Searching...
No Matches
Data Fields
SX1262_Handle Struct Reference

Hardware binding for a single SX1262 instance. More...

`#include <sx1262.h>`

## Data Fields
SPI_HandleTypeDef * | hspi
GPIO_TypeDef * | NSS_Port
uint16_t | NSS_Pin
GPIO_TypeDef * | RESET_Port
uint16_t | RESET_Pin
GPIO_TypeDef * | BUSY_Port
uint16_t | BUSY_Pin
GPIO_TypeDef * | DIO1_Port
uint16_t | DIO1_Pin
GPIO_TypeDef * | RXEN_Port
uint16_t | RXEN_Pin
GPIO_TypeDef * | TXEN_Port
uint16_t | TXEN_Pin

## Detailed Description

Hardware binding for a single SX1262 instance.

## Field Documentation

## ◆ BUSY_Pin

uint16_t SX1262_Handle::BUSY_Pin

## ◆ BUSY_Port

GPIO_TypeDef* SX1262_Handle::BUSY_Port

## ◆ DIO1_Pin

uint16_t SX1262_Handle::DIO1_Pin

## ◆ DIO1_Port

GPIO_TypeDef* SX1262_Handle::DIO1_Port

## ◆ hspi

SPI_HandleTypeDef* SX1262_Handle::hspi

## ◆ NSS_Pin

uint16_t SX1262_Handle::NSS_Pin

## ◆ NSS_Port

GPIO_TypeDef* SX1262_Handle::NSS_Port

## ◆ RESET_Pin

uint16_t SX1262_Handle::RESET_Pin

## ◆ RESET_Port

GPIO_TypeDef* SX1262_Handle::RESET_Port

## ◆ RXEN_Pin

uint16_t SX1262_Handle::RXEN_Pin

## ◆ RXEN_Port

GPIO_TypeDef* SX1262_Handle::RXEN_Port

## ◆ TXEN_Pin

uint16_t SX1262_Handle::TXEN_Pin

## ◆ TXEN_Port

GPIO_TypeDef* SX1262_Handle::TXEN_Port

The documentation for this struct was generated from the following file:

- SX1262/sx1262.h